# Neighbor View

Device > Configure > CDP Configuration > Neighbor View

The Neighbor View dialog box provides general information on the devices connected to this device. From here, you can access more detailed information on a particular neighbor device.

This dialog box displays the following data:

- Neighbor Device's Port (cdpCacheDevicePort)
- Device ID (cdpCacheDeviceId)
- Address (cdpCacheAddress)
- Hardware Platform (cdpCachePlatform)

The following list specifies buttons in this dialog box, as well as their function:

- Click Detail to launch the Neighbor Detail dialog box for the selected neighbor device.
- Click OK to continue.
- Click Apply to save the changes in the dialog box.
- Click Cancel to close the dialog box.
- Click Refresh to update the contents of the dialog box.
- Click Print to print the contents of the dialog box.
- Click Help to access online help.

Neighbor Device's Port (cdpCacheDevicePort)

Port identifier string, as reported in the most recent CDP message. This is typically the value of the corresponding ifName object. A zero-length string indicates that no Port ID field (TLV) was reported.

Device ID (cdpCacheDeviceId)

Device identifier string, as reported in the most recent CDP message. A zero-length string indicates that no Device ID field (TLV) was reported.

Address (cdpCacheAddress)

First network-layer address of the SNMP agent on the device, as reported in the most recent CDP message. For example, if the corresponding instance of cacheAddressType has the value "ip(1)", then this object is an IP address.

Hardware Platform (cdpCachePlatform)

Hardware platform of the device, as reported in the most recent CDP message. A zero-length string indicates that no Platform field (TLV) was reported.