# Configuration Information

To access the Configuration Information dialog box, right-click on a console or auxiliary port and select Configure.

This dialog box displays the following data:

- Active (tsLineActive)
- Type (tsLineType)
- Autobaud (tsLineAutobaud)
- Input Speed (tsLineSpeedin)
- Output Speed (tsLineSpeedout)
- Flow Control (tsLineFlow)
- Modem Control (tsLineModem)
- Location (tsLineLoc)
- Terminal Type (tsLineTerm)
- Idle Timeout (secs) (tsLineTmo)
- Sessions in Use (tsLineNses)
- TACACS User Name (tsLineUser)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.
- Click Apply to save the changes in the dialog box.
- Click Cancel to close the dialog box.
- Click Refresh to update the contents of the dialog box.
- Click Print to print the contents of the dialog box.
- Click Help to access online help.

Active (tsLineActive)

Indicates whether or not this line is active.

Type (tsLineType)

Type of line.

Autobaud (tsLineAutobaud)

Indicates whether or not the line will autobaud.

Input Speed (tsLineSpeedin)

Input speed the line is running at.

Output Speed (tsLineSpeedout)

Output speed the line is running at.

Flow Control (tsLineFlow)

Type of flow control the line is using.

Modem Control (tsLineModem)

Type of modem control the line is using.

Location (tsLineLoc)

Physical location of the line.

Terminal Type (tsLineTerm)

Terminal type of the line.

Idle Timeout (secs) (tsLineTmo)

Idle timeout interval for this line, in seconds.

Sessions in Use (tsLineNses)

Current number of sessions in use on this line.

TACACS User Name (tsLineUser)

If TACACS is enabled, the TACACS user name of the user on this line.