# System Information

Device > Configure > System Information

This dialog box provides general system information, displaying chassis, image, and entity information.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

> Chassis:

- Orderable Part Number (ceAssetOrderablePartNumber)
- Hardware Revision (ceAssetHardwareRevision)
- Part Number (ceAssetMfgAssyNumber)
- Board Revision (ceAssetMfgAssyRevision)
- Chassis Serial Number (ceAssetSerialNumber)

> System:

- IOS Version (IOS Version)
- IOS Feature Set (IOS Feature Set)
- IOS Sysdescr (IOS Sysdescr)
- ROM Monitor (romVersion)
- System Image (sysConfigName)
- Last Reload Reason (whyReload)

  Configuration Register:

- Current Value (configRegister)
- Value at Next Reload (configRegNext)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Chassis:

Orderable Part Number (ceAssetOrderablePartNumber)

Part number to use to when ordering the entity.

Hardware Revision (ceAssetHardwareRevision)

Hardware revision string for the entity.

Part Number (ceAssetMfgAssyNumber)

Manufacturing assembly number for the entity.

Board Revision (ceAssetMfgAssyRevision)

Revision string for the entity, within ceAssetMfgAssyNumber.

Chassis Serial Number (ceAssetSerialNumber)

Serial number of the entity.

System:

IOS Version (IOS Version)

Indicates what version of IOS is running on this device.

IOS Feature Set (IOS Feature Set)

Indicates the IOS feature set currently running on this device.

IOS Sysdescr (IOS Sysdescr)

Provides information on the version of IOS running on this device.

ROM Monitor (romVersion)

ROM monitor version.

System Image (sysConfigName)

Name of the system boot image.

Last Reload Reason (whyReload)

Reason for the last reload.

Configuration Register:

Current Value (configRegister)

Current value of the configuration register.

Value at Next Reload (configRegNext)

Value of the configuration register after the next reload.