# ARP Table

Device > Configure > ARP Table

The ARP Table dialog box lists IP addresses configured on this device and their corresponding physical addresses. From here, you can delete IP/physical address mappings.

This dialog box displays the following data:

- Interface (ipNetToMediaIfIndex)
- Network Address (ipNetToMediaNetAddress)
- Physical Address (ipNetToMediaPhysAddress)
- Type (ipNetToMediaType)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.
- Click Apply to save the changes in the dialog box.
- Click Cancel to close the dialog box.
- Click Delete to delete an existing IP/physical address mapping.
- Click Refresh to update the contents of the dialog box.
- Click Print to print the contents of the dialog box.
- Click Help to access online help.

Interface (ipNetToMediaIfIndex)

Interface on which the equivalence of this entry is effective.

Network Address (ipNetToMediaNetAddress)

IP address corresponding to the media-dependent physical address.

Physical Address (ipNetToMediaPhysAddress)

Media-dependent physical address.

Type (ipNetToMediaType)

Specifies the mapping type:

other (1) | none of the following
invalid (2) | invalid mapping
dynamic (3) | dynamic mapping
static (4) | static mapping

Note: Whether the agent removes an invalid mapping from ipNetToMediaTable is implementation–specific.