# SNMP Traffic

Device > Monitor > SNMP Traffic

From the SNMP Traffic dialog box, you can evaluate the performance of this device by monitoring SNMP traffic activity.

This dialog box displays the following data:

- Total In Request Objects (snmpInTotalReqVars)
- Total In Set Objects (snmpInTotalSetVars)
- In Get Requests (snmpInGetRequests)
- Out Get Requests (snmpOutGetRequests)
- Out Set Requests (snmpOutSetRequests)
- In Get Responses (snmpInGetResponses)
- Out Get Responses (snmpOutGetResponses)
- In Traps (snmpInTraps)
- Out Traps (snmpOutTraps)
- In GetNexts (snmpInGetNexts)
- Out GetNexts (snmpOutGetNexts)
- In Set Requests (snmpInSetRequests)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.
- Click Start/Stop to begin/end device monitoring.
  Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.
- Click Cancel to close the dialog box.
- Click Print to print the contents of the dialog box.
- Click Help to access online help.

Total In Request Objects (snmpInTotalReqVars)

Total number of MIB objects retrieved successfully by the SNMP protocol entity as a result of receiving valid SNMP Get-Request and Get-Next PDUs.

Total In Set Objects (snmpInTotalSetVars)

Total number of MIB objects altered successfully by the SNMP protocol entity as a result of receiving valid SNMP Set-Request PDUs.

In Get Requests (snmpInGetRequests)

Total number of SNMP Get-Request PDUs accepted and processed by the SNMP protocol entity.

Out Get Requests (snmpOutGetRequests)

Total number of SNMP Get-Request PDUs generated by the SNMP protocol entity.

Out Set Requests (snmpOutSetRequests)

Total number of SNMP Set-Request PDUs generated by the SNMP protocol entity.

In Get Responses (snmpInGetResponses)

Total number of SNMP Get-Response PDUs accepted and processed by the SNMP protocol entity.

Out Get Responses (snmpOutGetResponses)

Total number of SNMP Get-Response PDUs generated by the SNMP protocol entity.

In Traps (snmpInTraps)

Total number of SNMP Trap PDUs accepted and processed by the SNMP protocol entity.

Out Traps (snmpOutTraps)

Total number of SNMP Trap PDUs generated by the SNMP protocol entity.

In GetNexts (snmpInGetNexts)

Total number of SNMP Get-Next PDUs accepted and processed by the SNMP protocol entity.

Out GetNexts (snmpOutGetNexts)

Total number of SNMP Get-Next PDUs generated by the SNMP protocol entity.

In Set Requests (snmpInSetRequests)

Total number of SNMP Set-Request PDUs accepted and processed by the SNMP protocol entity.